	_______________________ Auto Repair
Per-tire inspection — tread depth, pressure, age, wear pattern, damage, TPMS
	Phone: ____________________
Email: ____________________
Address: __________________


TIRE INSPECTION CHECKLIST
	YEAR

	MAKE

	MODEL


	VIN

	LICENSE PLATE

	MILEAGE


	TECHNICIAN

	DATE

	RO #




■ Pass — within spec    ■ Needs Attention — monitor / service soon    ■ Fail — safety concern / repair now
Tread: 6/32" or more is good · 4/32" plan to replace · 2/32" replace now (legal minimum in most states).
	Check
	LF
	RF
	LR
	RR
	Spare

	Tread depth — inner (32nds)
	
	
	
	
	

	Tread depth — center (32nds)
	
	
	
	
	

	Tread depth — outer (32nds)
	
	
	
	
	

	Pressure — measured (psi)
	
	
	
	
	

	Pressure — door-jamb spec (psi)
	
	
	
	
	

	DOT date code (week / year)
	
	
	
	
	

	Wear pattern (even / inner / outer / center / cupping / feathering)
	
	
	
	
	

	Sidewall — cracks, bulges, cuts
	
	
	
	
	

	Tread — punctures, nails, separation
	
	
	
	
	

	Valve stem & cap
	
	
	
	
	

	TPMS sensor reporting
	
	
	
	
	

	Lug nuts torqued to spec
	
	
	
	
	



	Inspection Item
	Yes
	No
	Notes / Measurements

	RECOMMENDATIONS

	Rotation recommended
	☐
	☐
	

	Alignment recommended (uneven wear)
	☐
	☐
	

	Balance recommended (vibration)
	☐
	☐
	

	Replace — tread at or below 2/32" (wear bars)
	☐
	☐
	

	Replace — age over 6 years or sidewall damage
	☐
	☐
	



TIRE BRAND / SIZE / NOTES
	


Technician signature: ______________________          Customer signature: ______________________
Free template from garageauto.app  ·  Adapt it to your shop  ·  Not a substitute for state inspection requirements




