	_______________________ Automotive Workshop
Per-tyre inspection, tread depth, pressure, age, wear pattern, damage, TPMS
	Phone: ____________________
Email: ____________________
Address: __________________


TYRE INSPECTION CHECKLIST
	YEAR

	MAKE

	MODEL


	VIN

	REGO / STATE

	ODOMETER (KM)


	TECHNICIAN

	DATE (DD/MM/YYYY)

	JOB NO.




■ Pass — within spec    ■ Needs Attention — monitor / service soon    ■ Fail — safety concern / repair now
Tread: 4 mm or more is good · 3 mm plan to replace · replace at 1.5 mm, the minimum in the vehicle standards at the time of writing.
	Check
	LF
	RF
	LR
	RR
	Spare

	Tread depth, inner (mm)
	
	
	
	
	

	Tread depth, centre (mm)
	
	
	
	
	

	Tread depth, outer (mm)
	
	
	
	
	

	Pressure measured (psi / kPa)
	
	
	
	
	

	Tyre placard pressure (kPa / psi)
	
	
	
	
	

	Manufacture date code (week / year)
	
	
	
	
	

	Wear pattern (even / inner / outer / centre / cupping / feathering)
	
	
	
	
	

	Sidewall, cracks, bulges, cuts
	
	
	
	
	

	Tread, punctures, nails, separation
	
	
	
	
	

	Valve stem & cap
	
	
	
	
	

	TPMS (if fitted)
	
	
	
	
	

	Wheel nuts torqued to spec
	
	
	
	
	



	Inspection Item
	Yes
	No
	Notes / Measurements

	RECOMMENDATIONS

	Rotation recommended
	☐
	☐
	

	Wheel alignment recommended (uneven wear)
	☐
	☐
	

	Balance recommended (vibration)
	☐
	☐
	

	Replace, tread at or below 1.5 mm
	☐
	☐
	

	Replace, age over 6 years or sidewall damage
	☐
	☐
	



TYRE BRAND / SIZE / NOTES
	


Technician signature: ______________________          Customer signature: ______________________
Free template by garageauto.app/au  ·  Manage your job cards digitally  ·  A$54/month, 7 days free  ·  Not a substitute for a roadworthy inspection




