Car Service Schedule by Kilometres
Typical intervals, the manufacturer's service book always takes precedence
Use this as a planning guide. Intervals vary by make, engine and driving conditions. Where your service book gives a different interval, follow the book.
	Interval
	What is typically done

	Every 10,000 km or 6 months
	Engine oil & filter · tyre pressures & rotation · brake & fluid check · lights, wipers, battery

	Every 15,000 km or 12 months
	Standard service (above) + engine & cabin air filters · brake pads measured · safety inspection

	Every 30,000 km
	Above + fuel filter (if serviceable) · brake fluid flush · wheel alignment check · drive belt inspection

	Every 40,000 – 60,000 km
	Major service: spark plugs · coolant replace · transmission fluid (if scheduled) · diff oil · full inspection

	Every 80,000 – 100,000 km
	Above + timing belt if fitted (by km, non-negotiable) · water pump often done with it · suspension bushes reviewed

	Every 100,000 km +
	Repeat cycle · cooling system pressure test · battery (typically 3–5 years) · shocks & struts reviewed


THIS VEHICLE
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	Make / model / year


	Engine


	Service book interval




SERVICE RECORD
	Date
	Odometer (km)
	Service type
	Workshop
	Next due
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